QuickPlay Pro v1.7.5 (June 11, 2020)
- Fixed an issue where settings on Calculite IntelliHue were inadvertently being modified
- Updated serial number ranges for several CK and Vaya devices
- Added support for Archipoint RGBW
- Added support for ReachElite HO

QuickPlay Pro v1.7.4 (September 18, 2019)
- Fixed Resolution tab disabled for Reach Elite when serial # is found under Search.
- Fixed FW version not displayed for Graze MX4
- Fixed Smartjack Pro timing out of spec
- Fixed RDM ‘clear identify’ not sent when leaving fixture selection tab
- Fixed RDM fixture identify state on program exit
- Added support for Vaya Linear 4 channel
- Added support for Graze Compact
- Added support for PureStyle Compact
- Added support for iHue Downlight

QuickPlay Pro v1.7.3 (March 25, 2019)
- Added support for Vaya Flood LP10
- New icon and splash screen

QuickPlay Pro v1.7.0 (August 15, 2017)
- Fixed CM-150 image and naming
- Added support for Graze IntelliHue
- Added support for Reach Elite
- Added support for Accent 4C
- Fixed CM-150 fuse status at 7.5V and 12V

QuickPlay Pro v1.6.0 (March 15, 2017)
- Fixed CM-400 48V EO image and naming
- Updated product naming for PureStyle
- Fixed type on fixtures page
- Fixed Antumbra image and product information link
- Verified support for eW/eColor Burst gen2
- Updated Addressing and Configuration Guide

QuickPlay Pro v1.5.5 (July 13, 2016)
- Fixed PDS-400-48EO Image and naming convention
- Fix additional instances of Accent Compact naming convention
- Remove program all from Antumbra Keypad as it is not relevant
- Fixed bug with fixtures not having right number of channels in address fixtures window
- Correct additional instances of PureStyle naming convention
- Replaced Accent Compact Base Light Number with DMX Start Address
- Fixed bug with Accent Compact eW fixtures not correctly handing fixture identification
- Fixed White Point Optimization to only fixtures with capability and correct configuration
- Added support for eW Blast Gen4
- Added dates to the release notes file
- Updated Addressing and Configuration Guide

QuickPlay Pro v1.5.4 (February 22, 2016)
- Fixed bug with SmartJackPro data output
- Added support for Antumbra iColor and Ethernet Keypads
- Update name of Accent Compact
- Fixed a bug with ColorBurst parameter read back
- Added additional user configurable parameters for Burst and Burst Compact fixtures
- Fixed RDM Bulk Load capability

QuickPlay Pro v1.5.3 (February 1, 2016)
- Fixed OSX bug with iPlayer3 and SmartJackPro compatibility
- Added support for Reach 4Ch fixtures
- Map generation fix for DS-100ca, Vaya Control Module and Accent EC
- Fixed tab indexing new fixtures page
- General architectural cleanup 

QuickPlay Pro v1.5.2 (October 29, 2015)
- Fixed bug with Serial Port communication
- Added support for Blast gen4, Burst gen2, PureStyle, Accent EC fixtures
- Added support for eW Graze startup values
- Added support for eW Cove MX Precision Dimming
- Added additional configuration options for DS-100ca
- Update Qt framework to 5.x
- Moved Mac and Windows builds to 64 bit
- General architectural cleanup 
- Notes: 
	Currently NOT compatible with OS X El Capitan (10.11). Please ONLY use with OS X Yosemite (10.10). More updates on El Capitan compatibility to be available soon.

QuickPlay Pro v1.5.1 (July 13, 2015)
- Support added for Live Scan for more fixtures.
- Fix text bug on splash screen and help about screen
- Fix map file generation logic to not output chromasic ports with no nodes
- Support added for Vaya PDS and DS-100ca
- Fix tab indexing
- Notes: 
	- If you are installing QuickPlay over a previous version on Microsoft Windows, the installation process will not prompt you to remove the old version.
	- On OS X, having two or more displays of differing resolutions will cause the controller drop down list to detach from the main window in QuickPlayPro.

QuickPlay Pro v1.5.0
- Support added for Live Scan for more fixtures.
- Vaya Flood support.
- Intellipower has been removed and will be added in a future release.  Previous release can 
be used in the interim for Intellipower support.

QuickPlay Pro v1.4.15

Release Notes - v 1.4.15 build 
- Internal Release.
- Support added for Live Scan for Full Reach fixtures.
- Ability to toggle between 2 channel and 3 channel input mode for iW Reach Powercore.
- Abililty to read Live Scan property from Graze MX Powercore fixtures.
- Support added for eW / eColor Archipoint Powercore.
- Fix crashes in the Address Fixtures window.
- Fix crash when importing csv files.
- Fix text-alignment issues on Mac OS X.

QuickPlay Pro v1.4.14

Release Notes - v 1.4.14 build 
- Support added for Vaya Linear MP
- China serial numbers supported for Reach

QuickPlay Pro v1.4.13

Release Notes - v 1.4.13 build 20131119 (Mac OS X only)
- introduced support for Vaya fixtures.
- corrected slicing of the copyright notice in the ‘about QuickPlay Pro’ splash screen.
- Prevent the default FTDI kernel extension from opening connections to the iPlayer3 on OS X 10.9.
- Updated the FTDI kernel extension included in the application package

QuickPlay Pro v1.4.12

Release Notes - v 1.4.12 build 20130927
- Added fixture serial number range filtering to prevent using partial RDM serial numbers that are ambiguous with legacy cove fixture serial numbers.
- Added controls in the PDS Configuration/Data Enabler tab to support new IntelliPower Auto-Discovery parameters introduced into the DEPro Intellipower supply firmware (InteiilPower Data Receiver Count and Auto Discovery Attempts).
- Updated copyright information in about and splash screens.
- Updated setup project to InstallShield 2013.
-Added translation of RDM type fixture names to provide friendly product names to end users.
-Added product images for new Vaya products.

QuickPlay Pro v1.4.11

- Note: If you are installing QuickPlay over a previous version on Microsoft Windows, the installation process may take several minutes.
- Windows 7 users – add QuickPlay Pro to the Allowed Programs through Windows Firewall
- Launching QuickPlay Pro for the first time after an upgrade/fresh install will install FTD drivers

- IntelliPower supported only on Windows

Release Notes - v 1.4.11 build 20130516
-  New drivers necessary for iPlayer 3 communication installed when launching QuickPlay Pro for the first time (Windows)
-  Support for iW and iColor MR gen 3 fixtures
-  Support for PDS-60ca with Fail Over devices
-  Support for ItelliHue SkyRibbon fixtures
-  Support for iW/Color Graze EC/QLX/MX fixtures
-  Support for ColorGraze MX4 Powercore fixtures
-  Support for chromasync and startup colors for Archipoint fixtures with the latest firmware
-  Ability to set the subnet mask of IntelliPower devices with a custom firmware version
-  Increased network index range for IntelliPower Devices, adding ability to specify start and end search index as well as displaying which are the already occupied network indexes

Release Notes - v 1.4.10 build 20121210
- Adding support for Data Enabler IntelliPower and Data Receiver Intellipower

Release Notes - v 1.4.9 build 20121107
- Adding support for iColorCove EC/QLX Powercore

Release Notes - v 1.4.8 build 20120830
- Migrated Windows installer to InstallShield. This breaks the ability to automatically uninstall previous versions of this application. Users will need to uninstall the old version manually.
- Added support for Reach Compact fixtures
- Fixture Configuration frame displays images for Vaya fixtures
- Minor bug fixes

Release Notes – v1.4.7 build 20120515
- Added support for Archipoint
- Added startup colors for ColorBlast and ColorBurst Compact
- Added support for Powercore Power Module – 20/30 RGB/IW
- Bug fix to enable the PDS-60ca tabs in PDS Configuration when using iColorPlayer
- For advanced users only – added a script to export the MAC/IP addresses of all discovered supplies and a script to program the IP addresses of discovered supply by importing csv file

Release Notes – v1.4.6 build 20120103
- Added support for iColor Player
- Added reset to factory settings feature for ColorBlaze TRX and ColorBlastTRX
- Fixtures light up dim white in PDS Configuration

Release Notes – v1.4.5 build 20110811
- Added support for the new firmware version for Multi Protocol Converter – able to program KiNET Mode, DMX Base Address, Number of Ports, Lights per Port
- Added support for the new firmware version for ColorBlaze TRX – able to program Master/Slave Mode, Master Mode Output, KiNET Output Mode, KiNET Output Number of Ports, DMX Trigger, DMX Trigger Address, Intensity Channel
- Added support for the new firmware version for DataEnabler Pro – able to program the KiNET Protocol Version
- Added support for the new generation of ColorBlast/ iW Blast Powercore  
- Added support for iW Fuse Powercore
- Added ColorBlaze TRX and Multi Protocol Converter to auto update 
- Fixed a bug creating only 1 port for PDS-60CA Combo 24V before discovering the fixtures
- Fixed a bug displaying the wrong channels Cove MX occupied in Address Fixtures when in 2 channel mode
- Fixed a bug preventing Address Fixtures from programming the DMX addresses of fixtures that had their serial numbers imported from a .csv file and were added to the mapper. 
- Fixed a bug that was not lighting up the fixtures correctly while sorting in Address Fixtures if the serial numbers were imported from a .csv file

Release Notes - v1.4.4 build 20110201
- Added support for eW Accent Powercore
- Updated Accent Powercore UI; programs only changed values
- Fixed a bug preventing Address Fixtures from importing Accent Powercore and Blaze TRX serial numbers
- Fixed a bug discovering fixtures connected to Data Enabler Pro
- Fixed a small auto-update bug

Release Notes - v1.4.3 build 20101215
- Updated UI to match changes to ColorBlaze TRX UI

Release Notes - v1.4.2 build 20101206
- Fixed bug addressing iW Cove MX 2/3 channel mode

Release Notes - v1.4.1 build 20101103
- Added support for ColorBlaze TRX
- Added support for iW Cove MX - 8/16 bit mode, 2/3 channel mode
- Added support for iColor Cove MX - 8/16 bit mode

Release Notes - v1.3 build 20100604
- Supports ColorBlast TRX
- Supports Data Enabler Pro
- Bug fixes

Release Notes - v1.3 build 20100517
- Added support for Blast TRX

Release Notes - v1.2 build 20100426
- Added support for Data Enabler Pro
- Import/Export functionality improved
- Cove fixture family is now discovered correctly
- DMX mapper properly recognizes recently discovered fixtures
- Various bug fixes

Built with Qt 4.6.2W/Qt 4.6.3M